00000000000i[     ] Bochs x86 Emulator 2.1.1
00000000000i[     ]   February 08, 2004
00000000000i[     ] System configuration
00000000000i[     ]   processors: 1
00000000000i[     ]   A20 line support: yes
00000000000i[     ]   APIC support: yes
00000000000i[     ] CPU configuration
00000000000i[     ]   level: 6
00000000000i[     ]   fpu support: yes
00000000000i[     ]   paging support: yes, tlb enabled: yes
00000000000i[     ]   mmx support: yes
00000000000i[     ]   sse support: 2
00000000000i[     ]   v8086 mode support: yes
00000000000i[     ]   3dnow! support: yes
00000000000i[     ]   PAE support: yes
00000000000i[     ]   PGE support: yes
00000000000i[     ]   PSE support: yes
00000000000i[     ]   x86-64 support: yes
00000000000i[     ]   SEP support: no
00000000000i[     ] Optimization configuration
00000000000i[     ]   Guest2HostTLB support: no
00000000000i[     ]   RepeatSpeedups support: no
00000000000i[     ]   Icache support: no
00000000000i[     ]   Host Asm support: yes
00000000000i[MEM0 ] allocated memory at 00B50020. after alignment, vector=00B51000
00000000000i[MEM0 ] 64.00MB
00000000000i[MEM0 ] rom at 0xf0000/65536 ('bin/BIOS-bochs-2-processors')
00000000000i[MEM0 ] rom at 0xc0000/29664 ('bin/VGABIOS-lgpl-latest')
00000000000i[APIC?] local apic in  initializing
00000000000i[APIC0] 80686
00000000000i[CMOS ] Using local time for initial clock
00000000000i[CMOS ] Setting initial clock to: Sun Oct 24 15:12:11 2004 (time0=1098598331)
00000000000i[DMA  ] channel 4 used by cascade
00000000000i[DMA  ] channel 2 used by Floppy Drive
00000000000i[FDD  ] fd0: 'op.img' ro=0, h=2,t=80,spt=18
00000000000i[WGUI ] IME disabled
00000000000i[KMAP ] Loading keymap from 'bin/keymaps/x11-pc-us.map'
00000000000i[KMAP ] Loaded 168 symbols
00000000000i[VGA  ] interval=30000
00000000000i[VGA  ] VBE Bochs Display Extension Enabled
00000000000i[VTIME] using 'realtime pit' synchronization method
00000000000i[     ] init_mem of 'harddrv' plugin device by virtual method
00000000000i[     ] init_mem of 'keyboard' plugin device by virtual method
00000000000i[     ] init_mem of 'serial' plugin device by virtual method
00000000000i[     ] init_mem of 'parallel' plugin device by virtual method
00000000000i[     ] init_mem of 'extfpuirq' plugin device by virtual method
00000000000i[     ] init_dev of 'harddrv' plugin device by virtual method
00000000000i[HD   ] Boot device will be 'a'
00000000000i[HD   ] Floppy boot signature check is enabled
00000000000i[     ] init_dev of 'keyboard' plugin device by virtual method
00000000000i[KBD  ] will paste characters every 1000 keyboard ticks
00000000000i[     ] init_dev of 'serial' plugin device by virtual method
00000000000i[SER  ] com1 at 0x03f8 irq 4
00000000000i[     ] init_dev of 'parallel' plugin device by virtual method
00000000000i[PAR  ] parallel port 1 at 0x378 irq 7
00000000000i[     ] init_dev of 'extfpuirq' plugin device by virtual method
00000000000i[     ] reset of 'harddrv' plugin device by virtual method
00000000000i[     ] reset of 'keyboard' plugin device by virtual method
00000000000i[     ] reset of 'serial' plugin device by virtual method
00000000000i[     ] reset of 'parallel' plugin device by virtual method
00000000000i[     ] reset of 'extfpuirq' plugin device by virtual method
00000004325i[BIOS ]  rombios.c,v 1.103.2.2 2004/02/02 22:39:22 cbothamy Exp $
00000330074i[KBD  ] reset-disable command received
00000353367i[VBIOS] VGABios $Id: vgabios.c,v 1.38 2003/11/05 23:21:19 cbothamy Exp $
00000353598i[VGA  ] VBE known Display Interface b0c2
00000353683i[VGA  ] VBE known Display Interface b0c0
00000356628i[VBIOS] VBE Bios $Id: vbe.c,v 1.35 2003/11/03 20:57:01 vruppert Exp $
00000356743i[VGA  ] VBE known Display Interface b0c2
00000360000e[VGA  ] character height = 1, skipping text update
00000390000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00000405000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00000450000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00000559079i[VGA  ] VBE known Display Interface b0c2
00000646738e[HD   ] device set to 0 which does not exist
00000647031e[HD   ] device set to 1 which does not exist
00000782611i[BIOS ] *** int 15h function AX=5300, BX=0000 not yet supported!
00000782744i[VGA  ] VBE known Display Interface b0c2
00000825000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00000842973i[CPU0 ] WBINVD: (ignoring)
00000850731i[CPU0 ] MOV_RdCd: read of CR4
00000855000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00000873675e[CPU0 ] exception(): 3rd (13) exception with no resolution, shutdown status is 00h, resetting
00000878000i[BIOS ]  rombios.c,v 1.103.2.2 2004/02/02 22:39:22 cbothamy Exp $
00001210057i[KBD  ] reset-disable command received
00001233350i[VBIOS] VGABios $Id: vgabios.c,v 1.38 2003/11/05 23:21:19 cbothamy Exp $
00001233581i[VGA  ] VBE known Display Interface b0c2
00001233666i[VGA  ] VBE known Display Interface b0c0
00001236611i[VBIOS] VBE Bios $Id: vbe.c,v 1.35 2003/11/03 20:57:01 vruppert Exp $
00001236726i[VGA  ] VBE known Display Interface b0c2
00001290000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00001320000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00001439062i[VGA  ] VBE known Display Interface b0c2
00001526721e[HD   ] device set to 0 which does not exist
00001527014e[HD   ] device set to 1 which does not exist
00001662597i[BIOS ] *** int 15h function AX=5300, BX=0000 not yet supported!
00001662730i[VGA  ] VBE known Display Interface b0c2
00001710000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00001722959i[CPU0 ] WBINVD: (ignoring)
00001725000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00001730717i[CPU0 ] MOV_RdCd: read of CR4
00001753661e[CPU0 ] exception(): 3rd (13) exception with no resolution, shutdown status is 00h, resetting
00001757986i[BIOS ]  rombios.c,v 1.103.2.2 2004/02/02 22:39:22 cbothamy Exp $
00002090043i[KBD  ] reset-disable command received
00002113374i[VBIOS] VGABios $Id: vgabios.c,v 1.38 2003/11/05 23:21:19 cbothamy Exp $
00002113605i[VGA  ] VBE known Display Interface b0c2
00002113690i[VGA  ] VBE known Display Interface b0c0
00002116635i[VBIOS] VBE Bios $Id: vbe.c,v 1.35 2003/11/03 20:57:01 vruppert Exp $
00002116750i[VGA  ] VBE known Display Interface b0c2
00002160000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00002205000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00002319086i[VGA  ] VBE known Display Interface b0c2
00002406745e[HD   ] device set to 0 which does not exist
00002407038e[HD   ] device set to 1 which does not exist
00002542621i[BIOS ] *** int 15h function AX=5300, BX=0000 not yet supported!
00002542754i[VGA  ] VBE known Display Interface b0c2
00002595000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00002602983i[CPU0 ] WBINVD: (ignoring)
00002610000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00002610741i[CPU0 ] MOV_RdCd: read of CR4
00002633685e[CPU0 ] exception(): 3rd (13) exception with no resolution, shutdown status is 00h, resetting
00002638010i[BIOS ]  rombios.c,v 1.103.2.2 2004/02/02 22:39:22 cbothamy Exp $
00002970067i[KBD  ] reset-disable command received
00002993360i[VBIOS] VGABios $Id: vgabios.c,v 1.38 2003/11/05 23:21:19 cbothamy Exp $
00002993591i[VGA  ] VBE known Display Interface b0c2
00002993676i[VGA  ] VBE known Display Interface b0c0
00002996621i[VBIOS] VBE Bios $Id: vbe.c,v 1.35 2003/11/03 20:57:01 vruppert Exp $
00002996736i[VGA  ] VBE known Display Interface b0c2
00003045000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00003090000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00003199072i[VGA  ] VBE known Display Interface b0c2
00003286731e[HD   ] device set to 0 which does not exist
00003287024e[HD   ] device set to 1 which does not exist
00003422607i[BIOS ] *** int 15h function AX=5300, BX=0000 not yet supported!
00003422740i[VGA  ] VBE known Display Interface b0c2
00003465000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00003482969i[CPU0 ] WBINVD: (ignoring)
00003490727i[CPU0 ] MOV_RdCd: read of CR4
00003495000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00003513671e[CPU0 ] exception(): 3rd (13) exception with no resolution, shutdown status is 00h, resetting
00003517996i[BIOS ]  rombios.c,v 1.103.2.2 2004/02/02 22:39:22 cbothamy Exp $
00003850053i[KBD  ] reset-disable command received
00003873346i[VBIOS] VGABios $Id: vgabios.c,v 1.38 2003/11/05 23:21:19 cbothamy Exp $
00003873577i[VGA  ] VBE known Display Interface b0c2
00003873662i[VGA  ] VBE known Display Interface b0c0
00003876607i[VBIOS] VBE Bios $Id: vbe.c,v 1.35 2003/11/03 20:57:01 vruppert Exp $
00003876722i[VGA  ] VBE known Display Interface b0c2
00003930000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00003960000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00004079058i[VGA  ] VBE known Display Interface b0c2
00004166717e[HD   ] device set to 0 which does not exist
00004167010e[HD   ] device set to 1 which does not exist
00004302593i[BIOS ] *** int 15h function AX=5300, BX=0000 not yet supported!
00004302726i[VGA  ] VBE known Display Interface b0c2
00004350000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00004362955i[CPU0 ] WBINVD: (ignoring)
00004365000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00004370713i[CPU0 ] MOV_RdCd: read of CR4
00004393657e[CPU0 ] exception(): 3rd (13) exception with no resolution, shutdown status is 00h, resetting
00004397982i[BIOS ]  rombios.c,v 1.103.2.2 2004/02/02 22:39:22 cbothamy Exp $
00004730039i[KBD  ] reset-disable command received
00004753370i[VBIOS] VGABios $Id: vgabios.c,v 1.38 2003/11/05 23:21:19 cbothamy Exp $
00004753601i[VGA  ] VBE known Display Interface b0c2
00004753686i[VGA  ] VBE known Display Interface b0c0
00004756631i[VBIOS] VBE Bios $Id: vbe.c,v 1.35 2003/11/03 20:57:01 vruppert Exp $
00004756746i[VGA  ] VBE known Display Interface b0c2
00004800000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00004845000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00004959082i[VGA  ] VBE known Display Interface b0c2
00005046741e[HD   ] device set to 0 which does not exist
00005047034e[HD   ] device set to 1 which does not exist
00005182617i[BIOS ] *** int 15h function AX=5300, BX=0000 not yet supported!
00005182750i[VGA  ] VBE known Display Interface b0c2
00005235000i[WGUI ] dimension update x=640 y=400 fontheight=16 fontwidth=8 bpp=8
00005242979i[CPU0 ] WBINVD: (ignoring)
00005250000i[WGUI ] dimension update x=720 y=400 fontheight=16 fontwidth=9 bpp=8
00005250737i[CPU0 ] MOV_RdCd: read of CR4
00005273681e[CPU0 ] exception(): 3rd (13) exception with no resolution, shutdown status is 00h, resetting
00005278006i[BIOS ]  rombios.c,v 1.103.2.2 2004/02/02 22:39:22 cbothamy Exp $
00005312500p[WGUI ] >>PANIC<< POWER button turned off.
00005312500i[SYS  ] Last time is 1098598341
00005312500i[CPU0 ] real mode
00005312500i[CPU0 ] CS.d_b = 16 bit
00005312500i[CPU0 ] SS.d_b = 16 bit
00005312500i[CPU0 ] | EAX=00000064  EBX=0000003e  ECX=00000000  EDX=0000f000
00005312500i[CPU0 ] | ESP=0000fff2  EBP=0000fffa  ESI=00000000  EDI=00000500
00005312500i[CPU0 ] | IOPL=0 NV UP DI NG NZ NA PO NC
00005312500i[CPU0 ] | SEG selector     base    limit G D
00005312500i[CPU0 ] | SEG sltr(index|ti|rpl)     base    limit G D
00005312500i[CPU0 ] |  DS:0000( 0000| 0|  0) 00000000 0000ffff 0 0
00005312500i[CPU0 ] |  ES:0000( 0000| 0|  0) 00000000 0000ffff 0 0
00005312500i[CPU0 ] |  FS:0000( 0000| 0|  0) 00000000 0000ffff 0 0
00005312500i[CPU0 ] |  GS:0000( 0000| 0|  0) 00000000 0000ffff 0 0
00005312500i[CPU0 ] |  SS:0000( 0000| 0|  0) 00000000 0000ffff 0 0
00005312500i[CPU0 ] |  CS:f000( 0000| 0|  0) 000f0000 0000ffff 0 0
00005312500i[CPU0 ] | EIP=000004ef (000004ef)
00005312500i[CPU0 ] | CR0=0x60000010 CR1=0x00000000 CR2=0x00000000
00005312500i[CPU0 ] | CR3=0x00000000 CR4=0x00000000
00005312500i[     ] restoring default signal behavior
00005312500i[CTRL ] quit_sim called with exit code 1
